rnwmc driver V10.20b
for Windows Vista, 7, 8, 10 / 32 and 64 bit systems
-----------------------------------------------------------------
- not usable for Windows XP and earlier
- not usable for AMD Athlon Processors

In this version eventually problems because of Microsoft Spectre and Meltdown Updates are solved!
Also solved are problems with updates since April 2018 unser Win 7 / 10 shown by earlier versions of rnwmc!

Please respect:
For first time of installation this driver must be installed by calling KSetup9.exe!
Older Versions of the rnwmc driver must be uninstalled in the device manager and in the control panel - Programs
Reinstallation, maybe after card or slot change can be done by the button "Automatic installation".

Bitte beachten:
Der Treiber muss durch Aufruf von KSetup9.EXE installiert werden!
Bei einer Installation über den Gerätemanager oder bei einer "Automatischen Installation"
werden ansonsten die Geräte "Kitara RealTime Device" und "Kithara System Device" 
nicht installiert und der Treiber ist nicht brauchbar!
Wenn Windows eine Nachinstallation fordert z.B. bei Erkennung einer Steuerungsbaugruppe in einem anderen Slot,
dann ist die Automatische Installation ausreichend.
Falls frühere Versionen auf einem System installiert sind, müssen diese zuvor
über den Gerätemanager und danach ggf. über die "Installierten Programme" deinstalliert werden. Ansonsten verbleiben
störende Einträge in der Liste der installierten Programme.
